Nützliches

Tools

https://github.com/akaJes/marlin-config/releases | Marlin Config Tool

https://github.com/Elenedeath/HE3D-Firmware | Marlin FW f. HE3D

https://www.repetier.com/firmware/v100/index.php | Marlin Config Tool 2

http://hacker3000-data.bplaced.net/vspace.one/ | HACKER3000 Config / Testprints

Slicer:

https://ultimaker.com/en/products/ultimaker-cura-software

Alternative Slicer:

https://all3dp.com/de/1/3d-slicer-software-3d-drucker/

3D/STL/CAD Downloaden

https://www.thingiverse.com/

https://grabcad.com/

https://www.turbosquid.com/

https://www.myminifactory.com/

https://pinshape.com/

3D Drucker

Owner: vspace.one

DOCUMENT HERE

Prusa Sliecer Settings

Folgende Settings als *.ini datei speichern und in den slicer importiren <webcode name=„Default“ frameborder=0 width=100% scrolling=yes externalResources=„,“> # generated by PrusaSlicer 2.1.0 on 2019-12-30 at 16:32:56 UTC

[print:SpacePrinter] avoid_crossing_perimeters = 1 bottom_fill_pattern = rectilinear bottom_solid_layers = 3 bridge_acceleration = 0 bridge_angle = 0 bridge_flow_ratio = 1 bridge_speed = 30 brim_width = 4 clip_multipart_objects = 0 compatible_printers = compatible_printers_condition = complete_objects = 0 default_acceleration = 0 dont_support_bridges = 1 elefant_foot_compensation = 0 ensure_vertical_shell_thickness = 1 external_perimeter_extrusion_width = 0.6 external_perimeter_speed = 50% external_perimeters_first = 0 extra_perimeters = 1 extruder_clearance_height = 20 extruder_clearance_radius = 20 extrusion_width = 0.6 fill_angle = 45 fill_density = 25% fill_pattern = honeycomb first_layer_acceleration = 0 first_layer_extrusion_width = 200% first_layer_height = 0.35 first_layer_speed = 30 gap_fill_speed = 20 gcode_comments = 0 gcode_label_objects = 0 infill_acceleration = 0 infill_every_layers = 1 infill_extruder = 1 infill_extrusion_width = 0.6 infill_first = 0 infill_only_where_needed = 0 infill_overlap = 25% infill_speed = 45 inherits = interface_shells = 0 layer_height = 0.3 max_print_speed = 80 max_volumetric_speed = 0 min_skirt_length = 10 notes = only_retract_when_crossing_perimeters = 1 ooze_prevention = 0 output_filename_format = [input_filename_base].gcode overhangs = 1 perimeter_acceleration = 0 perimeter_extruder = 1 perimeter_extrusion_width = 0.6 perimeter_speed = 35 perimeters = 3 post_process = print_settings_id = raft_layers = 0 resolution = 0 seam_position = aligned single_extruder_multi_material_priming = 1 skirt_distance = 6 skirt_height = 1 skirts = 4 slice_closing_radius = 0.059 small_perimeter_speed = 15 solid_infill_below_area = 70 solid_infill_every_layers = 0 solid_infill_extruder = 1 solid_infill_extrusion_width = 0.6 solid_infill_speed = 20 spiral_vase = 0 standby_temperature_delta = -5 support_material = 0 support_material_angle = 0 support_material_auto = 1 support_material_buildplate_only = 0 support_material_contact_distance = 0.2 support_material_enforce_layers = 0 support_material_extruder = 1 support_material_extrusion_width = 0.52 support_material_interface_contact_loops = 0 support_material_interface_extruder = 1 support_material_interface_layers = 3 support_material_interface_spacing = 0 support_material_interface_speed = 100% support_material_pattern = rectilinear support_material_spacing = 2.5 support_material_speed = 30 support_material_synchronize_layers = 0 support_material_threshold = 0 support_material_with_sheath = 1 support_material_xy_spacing = 50% thin_walls = 1 threads = 6 top_fill_pattern = rectilinear top_infill_extrusion_width = 0.6 top_solid_infill_speed = 15 top_solid_layers = 3 travel_speed = 100 wipe_tower = 0 wipe_tower_bridging = 10 wipe_tower_rotation_angle = 0 wipe_tower_width = 60 wipe_tower_x = 180 wipe_tower_y = 140 xy_size_compensation = 0

[filament:SpacePrinter] bed_temperature = 65 bridge_fan_speed = 100 compatible_printers = compatible_printers_condition = compatible_prints = compatible_prints_condition = cooling = 1 disable_fan_first_layers = 0 end_filament_gcode = „; Filament-specific end gcode \n;END gcode for filament\n“ extrusion_multiplier = 1 fan_always_on = 1 fan_below_layer_time = 120 filament_colour = #29B2B2 filament_cooling_final_speed = 3.4 filament_cooling_initial_speed = 2.2 filament_cooling_moves = 4 filament_cost = 20 filament_density = 1 filament_deretract_speed = nil filament_diameter = 1.75 filament_load_time = 0 filament_loading_speed = 28 filament_loading_speed_start = 3 filament_max_volumetric_speed = 0 filament_minimal_purge_on_wipe_tower = 15 filament_notes = „“ filament_ramming_parameters = „120 100 6.6 6.8 7.2 7.6 7.9 8.2 8.7 9.4 9.9 10.0| 0.05 6.6 0.45 6.8 0.95 7.8 1.45 8.3 1.95 9.7 2.45 10 2.95 7.6 3.45 7.6 3.95 7.6 4.45 7.6 4.95 7.6“ filament_retract_before_travel = nil filament_retract_before_wipe = nil filament_retract_layer_change = nil filament_retract_length = 2 filament_retract_lift = nil filament_retract_lift_above = nil filament_retract_lift_below = nil filament_retract_restart_extra = nil filament_retract_speed = 40 filament_settings_id = „“ filament_soluble = 0 filament_toolchange_delay = 0 filament_type = PLA filament_unload_time = 0 filament_unloading_speed = 90 filament_unloading_speed_start = 100 filament_wipe = nil first_layer_bed_temperature = 65 first_layer_temperature = 215 inherits = max_fan_speed = 100 min_fan_speed = 85 min_print_speed = 10 slowdown_below_layer_time = 5 start_filament_gcode = „; Filament gcode\n“ temperature = 215

[printer:SpacePrinter] bed_custom_model = bed_custom_texture = bed_shape = 0x0,180×0,180×180,0x180 before_layer_gcode = between_objects_gcode = cooling_tube_length = 5 cooling_tube_retraction = 91.5 default_filament_profile = „“ default_print_profile = deretract_speed = 0 end_gcode = M104 S0 ; turn off temperature\nG28 X0 ; home X axis\nM84 ; disable motors\n extra_loading_move = -2 extruder_colour = „“ extruder_offset = 0x0 gcode_flavor = smoothie high_current_on_filament_swap = 0 host_type = octoprint inherits = layer_gcode = machine_max_acceleration_e = 10000,5000 machine_max_acceleration_extruding = 1500,1250 machine_max_acceleration_retracting = 1500,1250 machine_max_acceleration_x = 9000,1000 machine_max_acceleration_y = 9000,1000 machine_max_acceleration_z = 500,200 machine_max_feedrate_e = 120,120 machine_max_feedrate_x = 500,200 machine_max_feedrate_y = 500,200 machine_max_feedrate_z = 12,12 machine_max_jerk_e = 2.5,2.5 machine_max_jerk_x = 10,10 machine_max_jerk_y = 10,10 machine_max_jerk_z = 0.2,0.4 machine_min_extruding_rate = 0,0 machine_min_travel_rate = 0,0 max_layer_height = 0 max_print_height = 200 min_layer_height = 0.07 nozzle_diameter = 0.6 parking_pos_retraction = 92 print_host = 3d.int.vspace.one printer_model = printer_notes = printer_settings_id = printer_technology = FFF printer_variant = printer_vendor = printhost_apikey = 2D2CCD5E8FFB4FD886BE02010B849977 printhost_cafile = remaining_times = 0 retract_before_travel = 2 retract_before_wipe = 0% retract_layer_change = 0 retract_length = 3 retract_length_toolchange = 10 retract_lift = 0 retract_lift_above = 0 retract_lift_below = 0 retract_restart_extra = 0 retract_restart_extra_toolchange = 0 retract_speed = 40 serial_port = serial_speed = 250000 silent_mode = 1 single_extruder_multi_material = 0 start_gcode = G28 ; home all axes\nG1 Z5 F5000 ; lift nozzle\n toolchange_gcode = use_firmware_retraction = 0 use_relative_e_distances = 0 use_volumetric_e = 0 variable_layer_height = 1 wipe = 0 z_offset = 0

[presets] print = SpacePrinter sla_print = sla_material = printer = SpacePrinter filament = SpacePrinter

</webcode>

Nützliche G/M-Codes

Lüfter (Layerblower) starten/stoppen mit M106/M107

Druck pausieren/fortsetzen M600/M601

GCode als start.gcode in Cura Adden - Vor dem Druck

Start G-Code

;Prime the extruder
G92 E0
G1 F200 E3
G92 E0

End G-Code

M104 S0 ; Extruder Temp 0
M140 S0 ; Deb Temp 0
;Retract the filament
G92 E1
G1 E-1 F300
G28 X0 Y0
M84

Calibration G-Code

G90
M280PS10.6 ; Reset probe pin
G91
G1 Z30 ; Move 20 Up (relative)
G90;
G28 X Y ; Home X & Y (to min)
M280PS3.0 ; Deploy probe pin
M565 X-44.4 Y-26.1 Z0
G32 ; Probe the bed & enable compensation
G1 X44.4 Y26.1
G30 Z1.3
M280PS10.6 ; Deploy probe pin
M280PS7.0 ; Deploy probe pin
M500 ; SAVE compensation grid