Nützliches

Tools

https://github.com/akaJes/marlin-config/releases | Marlin Config Tool

https://github.com/Elenedeath/HE3D-Firmware | Marlin FW f. HE3D

https://www.repetier.com/firmware/v100/index.php | Marlin Config Tool 2

http://hacker3000-data.bplaced.net/vspace.one/ | HACKER3000 Config / Testprints

Slicer:

https://ultimaker.com/en/products/ultimaker-cura-software

Alternative Slicer:

https://all3dp.com/de/1/3d-slicer-software-3d-drucker/

3D/STL/CAD Downloaden

https://www.thingiverse.com/

https://grabcad.com/

https://www.turbosquid.com/

https://www.myminifactory.com/

https://pinshape.com/

3D Drucker

Drucker 2 (instructed only)

Owner: vspace.one

DOCUMENT HERE

Nützliche G/M-Codes

Lüfter (Layerblower) starten/stoppen mit M106/M107

Druck pausieren/fortsetzen M600/M601

GCode als start.gcode in Cura Adden - Vor dem Druck

Start G-Code

;Prime the extruder
G92 E0
G1 F200 E3
G92 E0

End G-Code

M104 S0 ; Extruder Temp 0
M140 S0 ; Deb Temp 0
;Retract the filament
G92 E1
G1 E-1 F300
G28 X0 Y0
M84

Calibration G-Code

G90
M280PS10.6 ; Reset probe pin
G91
G1 Z30 ; Move 20 Up (relative)
G90;
G28 X Y ; Home X & Y (to min)
M280PS3.0 ; Deploy probe pin
M565 X-44.4 Y-26.1 Z0
G32 ; Probe the bed & enable compensation
G1 X44.4 Y26.1
G30 Z1.3
M280PS10.6 ; Deploy probe pin
M280PS7.0 ; Deploy probe pin
M500 ; SAVE compensation grid